


INSTALLATION INSTRUCTIONS



ALUMINUM PLATE

ANY DOOR OR EXIT HATCH

1. INSTALL THE ALUMINUM PLATE FROM INSIDE OF THE KIT.

2. ALIGN ALL MOUNTING HOLES AND USE THE SUPPLIED HARDWARE; CARRIAGE BOLTS, WASHER AND NUTS TO SECURE IT IN PLACE.

3. ALL NUTS SHOULD BE INSTALLED AT OPPOSITE SIDE OF THE ALUMINUM PLATE.

NUT

WASHER

TITLE:

HAVIS, INC.

75 JACKSONVILLE RD, WARMINSTER, PA. 18974

1-800-524-9900

INSTALL INSTRUCTION

CARRIAGE BOLT

SIZE

**A**

**DO NOT SCALE DRAWING**

DWG. NO.

PT-A-922-INST

REV

10/22

WEIGHT (LB): 21.88 SCALE: 1:8 SHEET 1 OF 1